**EXPERIMENT NO-1:**

**Aim:** Write a program to display message using DOS interrupts.

**SOURCE CODE:**

data segment

msg db 0dh,0ah,"hello$"

data ends

code segment

assume cs:code,ds:data

start: mov ax,data

mov ds,ax

mov ah,09h

mov dx,offset msg

int 21h


mov ah,4ch

int 21h

code ends

end start

**OUTPUT:**

****